*Heading
** Job name: LoadingJob1 Model name: Model-1
** Generated by: Abaqus/CAE 6.14-1
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Part-1
*End Part
**
*Part, name=Part-2
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Part-1-1, part=Part-1
*Node
*Element, type=C3D8R
*Element, type=C3D6
*Element, type=C3D4
*Node
*Nset, nset=Part-1-1-RefPt_, internal
*Nset, nset=LoadingWedge
*Elset, elset=LoadingWedge, generate
*Nset, nset=NotLoadingWedge
*Elset, elset=NotLoadingWedge
** Section: Al_section
*Solid Section, elset=NotLoadingWedge, material=Al7475-T7351
** Section: Al_elastic_section
*Solid Section, elset=LoadingWedge, material=Al7475-T7351_elastic
*End Instance
**
*Instance, name=Part-2-1, part=Part-2
*Node
*Element, type=R3D4
*Element, type=R3D3
*Node
*Nset, nset=Part-2-1-RefPt_, internal
*Elset, elset=Part-2-1, generate
*End Instance
**
*Nset, nset=AllNodes, instance=Part-1-1, generate
*Nset, nset=ApproxCMODLLPoint1, instance=Part-1-1
*Nset, nset=ApproxCMODLLPoint2, instance=Part-1-1
*Elset, elset=CrackMouthCutRegion, instance=Part-1-1
*Nset, nset=CrackTipLine, instance=Part-1-1
*Elset, elset=CrackTipLine, instance=Part-1-1
*Elset, elset=ExtractSetComplete, instance=Part-1-1, generate
*Nset, nset=FixX1Set, instance=Part-1-1
*Elset, elset=ListModePoint, instance=Part-1-1
*Nset, nset=LoadingPoint, instance=Part-1-1
*Nset, nset=LoadingPointLine, instance=Part-1-1
*Elset, elset=LoadingPointLine, instance=Part-1-1, generate
*Nset, nset=PunchLoadPoint, instance=Part-2-1
*Nset, nset=SkimCutRegion, instance=Part-1-1
*Elset, elset=SkimCutRegion, instance=Part-1-1
*Nset, nset=SymmY1Set, instance=Part-1-1
*Elset, elset=SymmY1Set, instance=Part-1-1
*Nset, nset=SymmY2Set, instance=Part-1-1
*Elset, elset=SymmY2Set, instance=Part-1-1
*Nset, nset=SymmY3Set, instance=Part-1-1
*Elset, elset=SymmY3Set, instance=Part-1-1
*Nset, nset=SymmYNodes1, instance=Part-1-1
*Nset, nset=SymmYNodes2, instance=Part-1-1
*Nset, nset=SymmYNodes3, instance=Part-1-1
*Nset, nset=SymmYNodes4, instance=Part-1-1
*Nset, nset=SymmYNodes5, instance=Part-1-1
*Nset, nset=SymmYNodes6, instance=Part-1-1
*Nset, nset=SymmYNodes7, instance=Part-1-1
*Nset, nset=SymmYNodes8, instance=Part-1-1
*Nset, nset=SymmYNodes9, instance=Part-1-1
*Nset, nset=SymmYNodes10, instance=Part-1-1
*Nset, nset=SymmYNodes11, instance=Part-1-1
*Nset, nset=SymmYNodes12, instance=Part-1-1
*Nset, nset=SymmYNodes13, instance=Part-1-1
*Nset, nset=SymmYNodes14, instance=Part-1-1
*Nset, nset=SymmYNodes15, instance=Part-1-1
*Nset, nset=SymmYNodes16, instance=Part-1-1
*Nset, nset=SymmYNodes17, instance=Part-1-1
*Nset, nset=SymmYNodes18, instance=Part-1-1
*Nset, nset=SymmYNodes19, instance=Part-1-1
*Nset, nset=SymmYNodes20, instance=Part-1-1
*Nset, nset=SymmYNodes21, instance=Part-1-1
*Nset, nset=SymmYNodes22, instance=Part-1-1
*Nset, nset=SymmYNodes23, instance=Part-1-1
*Nset, nset=SymmYNodes24, instance=Part-1-1
*Nset, nset=SymmYNodes25, instance=Part-1-1
*Nset, nset=SymmYNodes26, instance=Part-1-1
*Nset, nset=SymmYNodes27, instance=Part-1-1
*Nset, nset=SymmYNodes28, instance=Part-1-1
*Nset, nset=SymmYNodes29, instance=Part-1-1
*Nset, nset=SymmYNodes30, instance=Part-1-1
*Nset, nset=SymmYNodes31, instance=Part-1-1
*Nset, nset=SymmYNodes32, instance=Part-1-1
*Nset, nset=SymmYNodes33, instance=Part-1-1
*Nset, nset=SymmYNodes34, instance=Part-1-1
*Nset, nset=SymmYNodes35, instance=Part-1-1
*Nset, nset=SymmYNodes36, instance=Part-1-1
*Nset, nset=SymmYNodes37, instance=Part-1-1
*Nset, nset=SymmYNodes38, instance=Part-1-1
*Nset, nset=SymmYNodes39, instance=Part-1-1
*Nset, nset=SymmYNodes40, instance=Part-1-1
*Nset, nset=SymmYNodes41, instance=Part-1-1
*Nset, nset=SymmYNodes42, instance=Part-1-1
*Nset, nset=SymmYNodes43, instance=Part-1-1
*Nset, nset=SymmYNodes44, instance=Part-1-1
*Nset, nset=SymmYNodes45, instance=Part-1-1
*Nset, nset=SymmYNodes46, instance=Part-1-1
*Nset, nset=SymmYNodes47, instance=Part-1-1
*Nset, nset=SymmYNodes48, instance=Part-1-1
*Nset, nset=SymmYNodes49, instance=Part-1-1
*Nset, nset=SymmYNodes50, instance=Part-1-1
*Nset, nset=SymmYNodes51, instance=Part-1-1
*Nset, nset=SymmYNodes52, instance=Part-1-1
*Nset, nset=SymmYNodes53, instance=Part-1-1
*Nset, nset=SymmYNodes54, instance=Part-1-1
*Nset, nset=SymmYNodes55, instance=Part-1-1
*Nset, nset=SymmYNodes56, instance=Part-1-1
*Nset, nset=SymmYNodes57, instance=Part-1-1
*Nset, nset=SymmYNodes58, instance=Part-1-1
*Nset, nset=SymmYNodes59, instance=Part-1-1
*Nset, nset=SymmYNodes60, instance=Part-1-1
*Nset, nset=SymmYNodes61, instance=Part-1-1
*Nset, nset=SymmYNodes62, instance=Part-1-1
*Nset, nset=SymmYNodes63, instance=Part-1-1
*Nset, nset=SymmYNodes64, instance=Part-1-1
*Nset, nset=SymmYNodes65, instance=Part-1-1
*Nset, nset=SymmYNodesCMOD5, instance=Part-1-1
*Nset, nset=SymmYNodesCMOD10, instance=Part-1-1
*Nset, nset=SymmYNodesCMOD15, instance=Part-1-1
*Nset, nset=SymmYNodesCMOD20, instance=Part-1-1
*Nset, nset=SymmYNodesCMODRemain, instance=Part-1-1
*Nset, nset=SymmYNodesSkimCutLigament, instance=Part-1-1
*Nset, nset=SymmZ1Set, instance=Part-1-1
*Elset, elset=SymmZ1Set, instance=Part-1-1
*Nset, nset=V0Point, instance=Part-1-1
*Elset, elset=_PunchMasterSurf_SPOS, internal, instance=Part-2-1, generate
*Surface, type=ELEMENT, name=PunchMasterSurf
_PunchMasterSurf_SPOS, SPOS
*Elset, elset=_SpecimenSlaveSurf_S5, internal, instance=Part-1-1
*Elset, elset=_SpecimenSlaveSurf_S4, internal, instance=Part-1-1
*Elset, elset=_SpecimenSlaveSurf_S3, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=SpecimenSlaveSurf
_SpecimenSlaveSurf_S5, S5
_SpecimenSlaveSurf_S4, S4
_SpecimenSlaveSurf_S3, S3
*Surface, type=NODE, name=LoadingPointLine_CNS_, internal
LoadingPointLine, 1.
*Rigid Body, ref node=Part-2-1.Part-2-1-RefPt_, elset=Part-2-1.Part-2-1
*Elset, elset=__T0_Part-1-1_M_S1, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=_T0_Part-1-1_M, internal
__T0_Part-1-1_M_S1, S1
*Elset, elset=__T0_Part-1-1_S_S3, internal, instance=Part-1-1
*Elset, elset=__T0_Part-1-1_S_S4, internal, instance=Part-1-1
*Elset, elset=__T0_Part-1-1_S_S1, internal, instance=Part-1-1
*Elset, elset=__T0_Part-1-1_S_S2, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T0_Part-1-1_S, internal
__T0_Part-1-1_S_S3, S3
__T0_Part-1-1_S_S4, S4
__T0_Part-1-1_S_S2, S2
__T0_Part-1-1_S_S1, S1
*Tie, name=_T0_Part-1-1, adjust=no
_T0_Part-1-1_S, _T0_Part-1-1_M
*Elset, elset=__T1_Part-1-1_M_S5, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T1_Part-1-1_M, internal
__T1_Part-1-1_M_S5, S5
*Elset, elset=__T1_Part-1-1_S_S4, internal, instance=Part-1-1
*Elset, elset=__T1_Part-1-1_S_S3, internal, instance=Part-1-1
*Elset, elset=__T1_Part-1-1_S_S1, internal, instance=Part-1-1
*Elset, elset=__T1_Part-1-1_S_S2, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T1_Part-1-1_S, internal
__T1_Part-1-1_S_S4, S4
__T1_Part-1-1_S_S3, S3
__T1_Part-1-1_S_S2, S2
__T1_Part-1-1_S_S1, S1
*Tie, name=_T1_Part-1-1, adjust=no
_T1_Part-1-1_S, _T1_Part-1-1_M
*Elset, elset=__T2_Part-1-1_M_S4, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=_T2_Part-1-1_M, internal
__T2_Part-1-1_M_S4, S4
*Elset, elset=__T2_Part-1-1_S_S3, internal, instance=Part-1-1
*Elset, elset=__T2_Part-1-1_S_S2, internal, instance=Part-1-1
*Elset, elset=__T2_Part-1-1_S_S4, internal, instance=Part-1-1
*Elset, elset=__T2_Part-1-1_S_S1, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T2_Part-1-1_S, internal
__T2_Part-1-1_S_S3, S3
__T2_Part-1-1_S_S2, S2
__T2_Part-1-1_S_S4, S4
__T2_Part-1-1_S_S1, S1
*Tie, name=_T2_Part-1-1, adjust=no
_T2_Part-1-1_S, _T2_Part-1-1_M
*Elset, elset=__T3_Part-1-1_M_S6, internal, instance=Part-1-1, generate
*Surface, type=ELEMENT, name=_T3_Part-1-1_M, internal
__T3_Part-1-1_M_S6, S6
*Elset, elset=__T3_Part-1-1_S_S4, internal, instance=Part-1-1
*Elset, elset=__T3_Part-1-1_S_S1, internal, instance=Part-1-1
*Elset, elset=__T3_Part-1-1_S_S2, internal, instance=Part-1-1
*Elset, elset=__T3_Part-1-1_S_S3, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T3_Part-1-1_S, internal
__T3_Part-1-1_S_S4, S4
__T3_Part-1-1_S_S1, S1
__T3_Part-1-1_S_S2, S2
__T3_Part-1-1_S_S3, S3
*Tie, name=_T3_Part-1-1, adjust=no
_T3_Part-1-1_S, _T3_Part-1-1_M
*Elset, elset=__T4_Part-1-1_M_S3, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T4_Part-1-1_M, internal
__T4_Part-1-1_M_S3, S3
*Elset, elset=__T4_Part-1-1_S_S2, internal, instance=Part-1-1
*Elset, elset=__T4_Part-1-1_S_S3, internal, instance=Part-1-1
*Elset, elset=__T4_Part-1-1_S_S1, internal, instance=Part-1-1
*Elset, elset=__T4_Part-1-1_S_S4, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T4_Part-1-1_S, internal
__T4_Part-1-1_S_S2, S2
__T4_Part-1-1_S_S3, S3
__T4_Part-1-1_S_S4, S4
__T4_Part-1-1_S_S1, S1
*Tie, name=_T4_Part-1-1, adjust=no
_T4_Part-1-1_S, _T4_Part-1-1_M
*Elset, elset=__T5_Part-1-1_M_S3, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T5_Part-1-1_M, internal
__T5_Part-1-1_M_S3, S3
*Elset, elset=__T5_Part-1-1_S_S4, internal, instance=Part-1-1
*Elset, elset=__T5_Part-1-1_S_S3, internal, instance=Part-1-1
*Elset, elset=__T5_Part-1-1_S_S2, internal, instance=Part-1-1
*Elset, elset=__T5_Part-1-1_S_S1, internal, instance=Part-1-1
*Surface, type=ELEMENT, name=_T5_Part-1-1_S, internal
__T5_Part-1-1_S_S4, S4
__T5_Part-1-1_S_S3, S3
__T5_Part-1-1_S_S2, S2
__T5_Part-1-1_S_S1, S1
*Tie, name=_T5_Part-1-1, adjust=no
_T5_Part-1-1_S, _T5_Part-1-1_M
** Constraint: Constraint-1
*Coupling, constraint name=Constraint-1, ref node=LoadingPoint, surface=LoadingPointLine_CNS_
*Kinematic
2, 2
*End Assembly
**
** MATERIALS
**
** Aluminium alloy 7075-T6
*Material, name=Al7475-T7351
*Elastic
69150., 0.33
*Plastic
 447.4,   0.
 466.7, 0.01
 486.9, 0.02
  523., 0.04
 545.4, 0.06
  559., 0.09
  616., 0.13
*Material, name=Al7475-T7351_elastic
*Elastic
69150., 0.33
**
** INTERACTION PROPERTIES
**
*Surface Interaction, name=IntProp-1
1.,
*Friction, slip tolerance=0.005
 0.5,
*Surface Behavior, pressure-overclosure=HARD
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_1 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes1, YSYMM
** Name: SymmY1_2 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes2, YSYMM
** Name: SymmY1_3 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes3, YSYMM
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes4, YSYMM
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesCMODRemain, YSYMM
** Name: SymmY1_SkimCutLigament Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmYNodesSkimCutLigament, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary
SymmZ1Set, ZSYMM
**
** INTERACTIONS
**
** Interaction: SpecimenPunchContact
*Contact Pair, interaction=IntProp-1, type=SURFACE TO SURFACE, adjust=0.0
SpecimenSlaveSurf, PunchMasterSurf
** ----------------------------------------------------------------
**
** STEP: Lower
**
*Step, name=Lower, nlgeom=NO
*Static
0.1, 1., 1e-05, 1.
**
** LOADS
**
** Name: PunchLoad   Type: Concentrated force
*Cload
PunchLoadPoint, 3, -38500.
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: Raise
**
*Step, name=Raise, nlgeom=NO
*Static
0.01, 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: PunchDisp Type: Displacement/Rotation
*Boundary
PunchLoadPoint, 3, 3, 1.
**
** LOADS
**
** Name: PunchLoad   Type: Concentrated force
*Cload, op=NEW
**
** OUTPUT REQUESTS
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
coord, S
*El Print, Elset = ExtractSetComplete, Position = Integration Points, Frequency=999999
coord, S
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
coord, EE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PEEQ
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
SENER
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PENER
*Node Print, Nset = AllNodes, Frequency=999999
coord, U
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: RemoveEls
**
*Step, name=RemoveEls, nlgeom=NO
*Static
0.1, 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes1, YSYMM
** Name: SymmY1_2 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes2, YSYMM
** Name: SymmY1_3 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes3, YSYMM
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes4, YSYMM
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmY1_SkimCutLigament Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** INTERACTIONS
**
** Interaction: CrackMouthCut
*Model Change, remove
CrackMouthCutRegion,
** Interaction: SkimCut
*Model Change, remove
SkimCutRegion,
** Interaction: SpecimenPunchContact
*Model Change, type=CONTACT PAIR, remove
SpecimenSlaveSurf, PunchMasterSurf
**
** OUTPUT REQUESTS
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
coord, S
*El Print, Elset = ExtractSetComplete, Position = Integration Points, Frequency=0
coord, S
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
coord, EE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
PE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
PEEQ
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
SENER
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=0
PENER
*Node Print, Nset = AllNodes, Frequency=0
coord, U
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: DummyStep
**
*Step, name=DummyStep, nlgeom=NO
*Static
0.2, 1., 1e-05, 0.2
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_1
**
*Step, name=ReleaseSymmY1_1, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_2 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes2, YSYMM
** Name: SymmY1_3 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes3, YSYMM
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes4, YSYMM
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_2
**
*Step, name=ReleaseSymmY1_2, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_2 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_3 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes3, YSYMM
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes4, YSYMM
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_3
**
*Step, name=ReleaseSymmY1_3, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_3 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes4, YSYMM
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_4
**
*Step, name=ReleaseSymmY1_4, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_4 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes5, YSYMM
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_5
**
*Step, name=ReleaseSymmY1_5, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_5 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes6, YSYMM
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_6
**
*Step, name=ReleaseSymmY1_6, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_6 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes7, YSYMM
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_7
**
*Step, name=ReleaseSymmY1_7, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_7 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes8, YSYMM
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_8
**
*Step, name=ReleaseSymmY1_8, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_8 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes9, YSYMM
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_9
**
*Step, name=ReleaseSymmY1_9, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_9 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes10, YSYMM
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_10
**
*Step, name=ReleaseSymmY1_10, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes11, YSYMM
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_11
**
*Step, name=ReleaseSymmY1_11, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_11 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes12, YSYMM
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_12
**
*Step, name=ReleaseSymmY1_12, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_12 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes13, YSYMM
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_13
**
*Step, name=ReleaseSymmY1_13, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_13 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes14, YSYMM
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_14
**
*Step, name=ReleaseSymmY1_14, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_14 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes15, YSYMM
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_15
**
*Step, name=ReleaseSymmY1_15, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes16, YSYMM
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_16
**
*Step, name=ReleaseSymmY1_16, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_16 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes17, YSYMM
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_17
**
*Step, name=ReleaseSymmY1_17, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_17 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes18, YSYMM
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_18
**
*Step, name=ReleaseSymmY1_18, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_18 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes19, YSYMM
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_19
**
*Step, name=ReleaseSymmY1_19, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_19 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes20, YSYMM
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_20
**
*Step, name=ReleaseSymmY1_20, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes21, YSYMM
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_21
**
*Step, name=ReleaseSymmY1_21, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_21 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes22, YSYMM
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_22
**
*Step, name=ReleaseSymmY1_22, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_22 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes23, YSYMM
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_23
**
*Step, name=ReleaseSymmY1_23, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_23 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes24, YSYMM
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_24
**
*Step, name=ReleaseSymmY1_24, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_24 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes25, YSYMM
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_25
**
*Step, name=ReleaseSymmY1_25, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_25 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes26, YSYMM
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_26
**
*Step, name=ReleaseSymmY1_26, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_26 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes27, YSYMM
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_27
**
*Step, name=ReleaseSymmY1_27, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_27 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes28, YSYMM
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_28
**
*Step, name=ReleaseSymmY1_28, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_28 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes29, YSYMM
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_29
**
*Step, name=ReleaseSymmY1_29, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_29 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes30, YSYMM
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_30
**
*Step, name=ReleaseSymmY1_30, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_30 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes31, YSYMM
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_31
**
*Step, name=ReleaseSymmY1_31, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_31 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes32, YSYMM
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_32
**
*Step, name=ReleaseSymmY1_32, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_32 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes33, YSYMM
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_33
**
*Step, name=ReleaseSymmY1_33, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_33 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes34, YSYMM
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ReleaseSymmY1_34
**
*Step, name=ReleaseSymmY1_34, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_34 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes35, YSYMM
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ListModePoint
**
*Output, history
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad1
**
*Step, name=ApplyLoad1, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad2
**
*Step, name=ApplyLoad2, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_35 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes36, YSYMM
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad3
**
*Step, name=ApplyLoad3, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_36 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes37, YSYMM
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad4
**
*Step, name=ApplyLoad4, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_37 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes38, YSYMM
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad5
**
*Step, name=ApplyLoad5, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_38 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes39, YSYMM
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad6
**
*Step, name=ApplyLoad6, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_39 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes40, YSYMM
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad7
**
*Step, name=ApplyLoad7, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_40 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes41, YSYMM
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad8
**
*Step, name=ApplyLoad8, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_41 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes42, YSYMM
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad9
**
*Step, name=ApplyLoad9, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_42 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodes43, YSYMM
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad10
**
*Step, name=ApplyLoad10, nlgeom=NO
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary, op=NEW
LoadingPoint, 2, 2, 0.0791
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_43 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD5, YSYMM
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
coord, S
*El Print, Elset = ExtractSetComplete, Position = Integration Points, Frequency=999999
coord, S
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
coord, EE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PE
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PEEQ
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
SENER
*El Print, Elset = ExtractSetComplete, Position = Centroidal, Frequency=999999
PENER
*Node Print, Nset = AllNodes, Frequency=999999
coord, U
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad11
**
*Step, name=ApplyLoad11, nlgeom=NO, inc=1000
*Static
0.1, 1., 1e-05, 0.1
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary
LoadingPoint, 2, 2, 0.2642
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad12
**
*Step, name=ApplyLoad12, nlgeom=NO, inc=1000
*Static
0.1, 1., 1e-05, 0.1
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary, op=NEW
LoadingPoint, 2, 2, 0.37011
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_CMOD05 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD10, YSYMM
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad13
**
*Step, name=ApplyLoad13, nlgeom=NO, inc=1000
*Static
0.1, 1., 1e-05, 0.1
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary, op=NEW
LoadingPoint, 2, 2, 0.65053
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_CMOD10 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD15, YSYMM
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad14
**
*Step, name=ApplyLoad14, nlgeom=NO, inc=1000
*Static
0.1, 1., 1e-05, 0.1
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary, op=NEW
LoadingPoint, 2, 2, 0.90756
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_CMOD15 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMOD20, YSYMM
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step
** ----------------------------------------------------------------
**
** STEP: ApplyLoad15
**
*Step, name=ApplyLoad15, nlgeom=NO, inc=1000
*Static
0.1, 1., 1e-05, 0.1
**
** BOUNDARY CONDITIONS
**
** Name: CMOD Type: Displacement/Rotation
*Boundary, op=NEW
LoadingPoint, 2, 2, 1.1617
** Name: FixX Type: Displacement/Rotation
*Boundary, op=NEW
FixX1Set, 1, 1
** Name: PunchDisp Type: Displacement/Rotation
*Boundary, op=NEW
PunchLoadPoint, 1, 1
PunchLoadPoint, 2, 2
PunchLoadPoint, 3, 3, 1.
PunchLoadPoint, 4, 4
PunchLoadPoint, 5, 5
PunchLoadPoint, 6, 6
** Name: SymmY1_CMOD20 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
** Name: SymmY1_CMODRemain Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmYNodesCMODRemain, YSYMM
** Name: SymmZ1 Type: Symmetry/Antisymmetry/Encastre
*Boundary, op=NEW
SymmZ1Set, ZSYMM
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
E, EE, PE, PEEQ, PEMAG, S
*Contact Output
CDISP, CSTRESS
**
** HISTORY OUTPUT: ApproxCMODLLPoint1
**
*Output, history
*Node Output, nset=ApproxCMODLLPoint1
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ApproxCMODLLPoint2
**
*Node Output, nset=ApproxCMODLLPoint2
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: ListModePoint
**
*Element Output, elset=ListModePoint
E11, E12, E13, E22, E23, E33, EE11, EE12, EE13, EE22, EE23, EE33, EEP, EP, INV3, PE11
PE12, PE13, PE22, PE23, PE33, PEEQ, PEP, PRESS, S11, S12, S13, S22, S23, S33, SP, TRESC
**
** HISTORY OUTPUT: LoadPin
**
*Node Output, nset=LoadingPoint
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: V0Point
**
*Node Output, nset=V0Point
CF1, CF2, CF3, CM1, CM2, CM3, RF1, RF2
RF3, RM1, RM2, RM3, U1, U2, U3, UR1
UR2, UR3
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step